Copyright 2022 ADVANCED MICRO DEVICES, INC. All Rights Reserved. 

AMD RAID controller Driver distribution list
Revision: 9.3.2.00130
Built date: 06/28/2022
OS: Windows10 x64, Windows11 21H2 x64, Windows11 22H2 x64

AMD-RAID binary file name:
	Windows UWP:
•	RAIDXpert2 UWP application
•	RAIDXpert2 Security Certificate
•	RAIDXpert2 Personal Information Exchange

RAIDXPert2 Application:
•	Setup.exe
•	Rcadm.exe
	
Known issues
•	RXP2 and rcadm.exe showing both xb000 and CC for PCIe Device Id.
•	Application not launching when OS username contains non-Latin character. 

Revision History
9.3.2.00130
•	NA
9.3.2.00127
•	Added Gen5 NVMe supported flags.
9.3.2.00121
•	No Changes
9.3.2.00118
•	SMART log information removed for the older logs.
•	RXP2 may freeze when array is in critical / offline state. 
9.3.2.00099
•	Added support for increase in number of RAID Array, Storage Controller, Disks
•	Enabled support for SMART status query for NVMe and SATA Drives.
9.3.0.00296
•	Added RXP2 GUI error messages.

9.3.0.00266
•	Fix for BSOD during clear metadata
•	Fix for SMART info on specific Model of NVMe
•	Added detailed help Strings to the RXP2 GUI when user unable to create array
•	RaidXpert2 User Guide updated

9.3.0.00245
•	Fix for rcpopup issue while running rebooter cycle.

9.3.0.00237
•	Fix for Negative (-ve) reading for temperature value.
•	Fix for Power Hours and Power cycle value.

9.3.0.00230
•	Added support for drive SMART information.

9.3.0.00206
•	Fix Don't list Physical Devices assigned as spares to Initialize Disk.
•	Fix rcadm.exe to update spare state after clear meta data operation.

9.3.0.00198
•	Added clear metadata feature to clear the raid metadata information.